Consolideck® DailyKlean Cleaning Specification

Specifier Note: The information provided below is intended to guide the Architect in developing specifications for products manufactured by PROSOCO, Inc. and should not be viewed as a complete source of information about the product(s). The Architect should always refer to the Product Data Sheet and MSDS for additional recommendations and for safety information.

Specifier Note: Paragraph below is for PART 1 GENERAL, Quality Assurance.

# TEST AREA

Test a minimum 4 ft. by 4 ft. area on each type of masonry. Use manufacturer’s application instructions. Let the test panel dry 3 to 7 days before inspection. Keep test panels available for comparison throughout the cleaning project.

Specifier Note: Paragraphs below are for PART 2 PRODUCTS, Manufacturers and Products.

# MANUFACTURER

PROSOCO, Inc., 3741 Greenway Circle, Lawrence, KS 66046. Phone: (800) 255-4255; Fax: (785) 830-9797. E-mail: CustomerCare@prosoco.com

# PRODUCT DESCRIPTION

Consolideck® DailyKlean is a specially designed, fragrance-free, concentrated maintenance cleaner for concrete floors, including floors treated with lithium-silicate hardening/densifying products. Though specifically designed for lithium-silicate hardened and densified floors, DailyKlean is an effective maintenance cleaner for almost any concrete floor. The specialized blend of degreasers and detergents removes most common soiling found on concrete floors. Recognized by the US EPA’s Safer Choice program and formulated to be safer for workers and the environment.

# TYPICAL TECHNICAL DATA

FORM: colorless, cloudy liquid

SPECIFIC GRAVITY: 0.999

pH: 8.6

WEIGHT/GALLON: 8.32 pounds

ACTIVE CONTENT: not applicable

TOTAL SOLIDS: not applicable

VOC CONTENT: 0

FLASH POINT: greater than 200 degrees F (greater than 93 degrees C) ASTM D 3278

FREEZE POINT: 31 degrees F (-1 degrees C)

SHELF LIFE: 2 years in tightly sealed, unopened container

VOC: Compliant with all national, state and district VOC regulations.

Specifier Note: Paragraphs below are for PART 3 EXECUTION, Installation.

# APPLICATION

Before applying, read “Preparation” and “Safety Information” sections in the Manufacturer’s Product Data Sheet for Consolideck® DailyKlean. Refer to the Product Data Sheet for additional information about application.

**Dilution**

For normal cleaning, dilute 1 ounce of cleaner per 1-gallon of fresh water.

For deep cleaning, dilute 2-ounces of cleaner per 1-gallon of fresh water.

For use with a Brightwell High Flow ECOMIX COMPACT dispenser unit:

* Ensure dispenser is set for I High Flow
* Dilution ratio of 128:1 at 1 ounce per gallon (8 milliliters per liter)

When set properly, Brightwell High Flow ECOMIX Compact dispenser’s chemical dilution dial will show the letter I at the top (in the 12:00 position). Read and follow all information and instructions included with the dispenser unit.

SPECIFIER NOTE: Do not use dilutions stronger than 4-ounces cleaner to 1-gallon of fresh water. Always use the mildest effective dilution possible.

SPECIFIER NOTE: For spot cleaning heavily soiled areas, begin testing DailyKlean at a dilution of 2-ounces of cleaner to 1-gallonf fresh water.

# Application Instructions

Apply with a mop or automatic scrubber. Rinsing is not necessary for routine surface cleaning. Mop up spent cleaner and dissolved contaminants, or allow automatic scrubber to vacuum it up. Do not let cleaner dry on the floor.

After deep-cleaning, or for cleaning in food processing areas, rinse well with fresh water. Do not let puddles or concentrated cleaner dry on the floor. Mop up rinse water, or vacuum up with auto scrubber.

SPECIFIER NOTE: Buff the cleaned floor with a white pad to increase the shine.

# Cleanup

Clean tools and equipment using fresh water.