Consolideck® DailyKlean ULTRA 15 Cleaning Specification

Specifier Note: The information provided below is intended to guide the Architect in developing specifications for products manufactured by PROSOCO, Inc. and should not be viewed as a complete source of information about the product(s). The Architect should always refer to the Product Data Sheet and MSDS for additional recommendations and for safety information

Specifier Note: Paragraph below is for PART 1 GENERAL, Quality Assurance.

# Test Area

Test a minimum 4 ft. by 4 ft. area of concrete. Use manufacturer’s application instructions. Let the test panel dry 3 to 7 days before inspection. Keep test panels available for comparison throughout the cleaning project.

Specifier Note: Paragraphs below are for PART 2 PRODUCTS, Manufacturers and Products.

# Manufacturer

PROSOCO, Inc., 3741 Greenway Circle, Lawrence, KS 66046. Phone: (800) 255-4255; Fax: (785) 830-9797. E-mail: CustomerCare@prosoco.com

# Product Description

Consolideck® DailyKlean ULTRA 15 is a highly concentrated, fragrance-free maintenance cleaner for concrete floors, including floors hardened and densified with lithium-silicate products. Though specifically designed for lithium-silicate hardened and densified floors, DailyKlean ULTRA 15 is an effective maintenance cleaner for almost any concrete floor. The specialized blend of degreasers and detergents removes most common soiling found on concrete floors. DailyKlean ULTRA 15 is ideal for use on warehouses, manufacturing plants, schools, stores, hospitals, restaurants and most any concrete floor. The product is sold in convenient tip-and-measure packaging to simplify proper measurement for use with 15-gallon auto-scrubber tanks. Recognized by the US EPA’s Safer Choice program. Formulated to be safer for workers and the environment.

# Typical Technical Data

FORM: colorless, cloudy liquid

SPECIFIC GRAVITY: 0.998

pH: 7.84

WEIGHT/GALLON: 8.30 pounds

ACTIVE CONTENT: not applicable

TOTAL SOLIDS: not applicable

VOC CONTENT: 0

FLASH POINT: greater than 200 degrees F (greater than 93 degrees C) ASTM D 3278

FREEZE POINT: 31 degrees F (-1 degrees C)

SHELF LIFE: 2 years in tightly sealed, unopened container

Specifier Note: Paragraphs below are for PART 3 EXECUTION, Installation.

# Application

Before applying, read “Preparation” and “Safety Information” sections in the Manufacturer’s Product Data Sheet for Consolideck® DailyKlean ULTRA 15. Refer to the Product Data Sheet for additional information about application.

**Dilution**

Dilute 4 ounces of cleaner per 15 gallons of fresh water.

**Application Instructions**

Apply with an automatic scrubber. Rinsing is not necessary for routine surface cleaning. Vacuum up spent cleaner and dissolved contaminants with automatic scrubber. Do not let puddles or concentrated cleaner dry on the floor.

After deep cleaning, or for cleaning in food-processing areas, rinse well with fresh water. Do not let puddles or concentrated cleaner dry on the floor. Vacuum up rinse water with automatic scrubber.

SPECIFIER NOTE: Buff the cleaned floor with a white pad to increase the shine.

# Cleanup

Clean tools and equipment using fresh water.