SECTION 09 51 13 – USG DONN® BRAND DXLA™ACOUSTICAL SUSPENSION SYSTEM

|  |
| --- |
| **Product Summary:**  |
| * Meets 2014 Guidelines for Health Care Facilities.
* 15/16" exposed, fire-rated system with aluminum cap.
* Capable of withstanding cleaning and/or disinfecting chemicals as tested in accordance with ASTM D5402.
* Suitable for use in food processing areas and meets USDA/FSIS requirements.
* Cross-tee override-ends resist twisting and give a professionally finished look.
* Proprietary QUICK-RELEASE™ cross tees.
* White gasket blends with grid and tile.
* ICC-ES evaluated for seismic installations (ICC-ESR-1222).
* Custom colors available
* **<insert product representative here>** or 800.874.4968 for technical questions
 |

|  |
| --- |
| **Note to Specifier:**  |
| * This document is not intended to function as a standalone specification. It is intended to assist the specifier in inserting the proper language into the following recommended specification sections:
	+ 09 51 13 Acoustical Panel Ceilings
	+ 09 51 23 Acoustical Tile Ceilings
	+ 09 51 33 Acoustical Metal Pan Ceilings
	+ 09 54 23 Linear Metal Ceilings
* The following IBC 2015 Sections Govern in addition to local code criteria for seismic ceilings:

Chapter 16 STRUCTURAL DESIGNChapter 17 SPECIAL INSPECTIONS AND TESTS* Language for seismic design, required reports and accessories are detailed in the specification section 01 40 00 QUALITY REQUIREMENTS.
* For more information regarding seismic design, please reference: <https://www.usg.com/content/usgcom/en/products-solutions/solutions/seismic.html>.
 |

1. GENERAL

Note to Specifier: If the specification is for a Seismic Application, add the following references to part 1.2B “related requirements”:

* + - * 1. Related Requirements:

ASTM C635 - Standard Specification for the Manufacture, Performance, and Testing of Metal Suspension Systems for Acoustical Tile and Lay-in Panel Ceilings.

ASTM C636 - Standard Practice for Installation of Metal Ceiling Suspension Systems for Acoustical Tile and Lay-in Panels.

ASTM E84 - Standard Method for Surface Burning Characteristics of Building Materials.

ASTM E580 - Standard Practice for Application of Ceiling Suspension Systems for Acoustical Tile and Lay-in Panels in Areas Subject to Earthquake Ground Motions.

2015 International Building Code - Section 1613, 1704, 1705, & 1706.

2013 California Building Code, chapters 8, 16, 16A and 25.

ASCE/SEI American Society of Civil Engineers 7-10: Minimum Design Loads for Buildings and Other Structures.

CISCA Ceilings & Interior Systems Construction Association.

Ceiling Systems Handbook

Seismic Construction Handbook

International Code Council ICC-ES Evaluation Report ESR-1222 issued December 2016.

Note to Specifier: If the specification is for a Seismic Application, add the following references to part 1.4 “informational submittals”. In Addition, require NVLAP certified reports to document acoustical performance.

* + - 1. INFORMATIONAL SUBMITTALS
				1. Product Test Reports: Provide test reports for each acoustical ceiling panel, performed by NVLAP certified testing agency.
				2. Evaluation Reports: For each ceiling suspension system, submit ICC-ES 1222 report showing compliance.
1. PRODUCTS

Note to Specifier: For Seismic applications, add the following criteria to “performance requirements”.

* + - 1. SEISMIC PERFORMANCE REQUIREMENTS
				1. Seismic Performance: Suspended grids and ceiling panels shall be installed in accordance to ASTM C636, ASTM E580 (including approved alternate methods).
				2. Ceiling design shall comply with ASCE/SEI American Society of Civil Engineers 7-10: Minimum Design Loads for Buildings and Other Structures

Note to Specifier: For DXLA Grid, insert the following language below.

2.5 METAL SUSPENSION SYSTEM FOR ACOUSTICAL CEILING PANEL

* + - * 1. Cold Rolled Steel Suspension System, UL Classified, **[Heavy Duty] [Intermediate Duty]** as defined by: ASTM C635; Double-web design; 15/16” (24 mm) exposed flange with pre-painted aluminum cap. Cross tee: cold roll-formed steel suspension system with double-web design with rectangular bulb; 15/16” (24 mm)exposed flange with pre-painted aluminum cap. **<INSERT DESIGNATION HERE>**:

Basis of Design: Subject to compliance with project requirements, the design is based on the following: USG Interiors, LLC, “USG DONN® Brand DXLA™ 15/16" Acoustical Suspension System.

Note: Main Tees for seismic applications must have a structural classification. For IBC category C use INTERMEDIATE DUTY and for IBC Category D E F use HEAVY DUTY. Adjust accessories to reflect relevant ceiling design criteria.

Structural Classification: **[intermediate duty] [heavy duty].**

Tee Profile: 15/16” (24 mm).

Tee Height: **[1 ½” (38 mm)] [1.64” (42 mm)].**

Grid Module: [As noted on drawings].

Fire Rating: [Class A] [Firecode].

**[standard flat white 050] [silver satin 002].**

Recycled Content: greater than 50%.

Note to Specifier: Retain paragraph below if the ceiling suspension is a seismic application, adjust structural classification above in #2 to match seismic criteria below:

Seismic Criteria:

Reference Seismic standards per ASTM E580 and CISCA guidelines.

Seismic Design Category as defined by the IBC (International Building Code): **[not applicable] [A-C] [D-F].**

* + - * 1. Accessories.

Wall molding: Inside Corner: Field-mitered joints at wall molding. Prefabricated corner cap; formed to 90° angle; hemmed edge; size and finish to match wall molding. Outside Corner: Prefabricated corner cap; formed to 90° angle; hemmed edge; size and finish to match wall molding.

Angle shape; 7/8” (22mm) thick mounting flange by 7/8” (22mm) thick face flange; hemmed edges; exposed surface pre-finished to match suspension system components. Available Product: **[M7Z] [M7A].**

Angle shape; 1” (25.4 mm) thick mounting flange by 1” (25.4 mm) thick face flange; hemmed edges; exposed surface pre-finished to match suspension system components. Available Product: MC11A25.

Note to Specifier: For Seismic category D E F applications use the paragraph below:

Angle shape; 2 in. mounting flange by 1 in. vertical flange; hemmed edges; exposed surface pre-finished to match suspension system components. Available Product: **[M20] [M20SM] [M20SM-2].**

Note to Specifier: For Alternate Seismic Solutions for categories C & D-F use the paragraph below:

Seismic Attachment Clip: Used to attach tees ends to perimeter angle for seismic design C D E F categories.

Available products: ACM7.

Molding Attachment Clip: 2 in. thick x 1/2 in. thick x 1-5/8 in.; for Fineline Suspension System. Used to attach cross tees and main tees to walls/ wall molding.

Molding Attachment Clip: 9/16 in. thick for SQ panels or FL panels, Available products: MAC2

Note to Specifier: For Seismic category D E F applications use the paragraphs below:

Seismic Separation joint accessories: Tee sleeves to accommodate movement: Snap fit sleeve, prefinished to match suspension system components.

For DX/DXL Fineline Suspension System; Available products: TFS-1.

Four way Seismic Separation joint clip: Connects 4 way intersection: Snap fit sleeve with optional screw/fixing holes.

Available products: DH4.

Compression Posts for bracing of ceiling applications:

Available products: Adjustable 18” to 30” **[VSA 18/30]**, Adjustable 30” to 48” [VSA 30/48], Adjustable 48” to 84” **[VSA 48/84]**, Adjustable 84” to 102” **[VSA 84/102]**, Adjustable 102” to 120” **[VSA 102/120]**, Adjustable 120” to 144” **[VSA 102/144]**.

* + - * 1. Suspension System Attachment devices.

Hanger Wire: Galvanized carbon steel; soft temper; pre-stretched; yield stress load at least three times the design load but not less than 12-gauge.

Spacing and gauge per IBC, UL and CISCA design.

Supplied and installed by ceilings subcontractor.

Disclaimer: The USG Product Specifications contained herein are intended for use as product reference material by architects, engineers, other design professionals, contractors, building code officials, or other competent construction industry trade professionals having an interest in the selection, specification and use of products manufactured by the subsidiaries of USG Corporation. The Specifications are intended solely as technical support incident to the sale and use of USG products and not intended to be a substitute for the design review and approval of the licensed design professionals for the project. These materials may be printed and/or transferred electronically solely as needed by the user. Because electronic text files can be modified by other parties, without notice or indication of such modifications, modification of USG Product Guide Specifications and Drawings is the sole responsibility of the Design Professional.